Small Board:

MotorA

PF0/ PWM0/UP switch

PE0

MotorB

PF1/ PWM1/DOWN switch

PE1

Tach

PB0/ CCP0

PB1/ CCP2

Ping

CCP1

Big Board:

IR Sensors

ADC0

ADC1

ADC2

Bumper switches, mode config:

PB0/PWM2

PB1/PWM3

PB2/SCL

PB3/SDA

Or whatever….