Updated 4/4/2011 by Katy

Small Board:

MotorA

PF0/ PWM0/UP switch -> connected to the yellow wire

PE0 -> orange wire

MotorB

PF1/ PWM1/DOWN switch -> purple wire

PE1 -> blue wire

Tach

PB0/ CCP0

PB1/ CCP2

Big Board:

Ping

CCP0

IR Sensors

ADC0

ADC1

ADC2

Bumper switches:

PB0/PWM2

PB1/PWM3

PB2/SCL

PB3/SDA

PC4/PHA0

PC5

PC6/PHB0

PC7